| Cisco can either support the user's authorization request to access the local server or it can pass the request to a remote server. Small networks can authorize users on the NAS, which stores usernames and passwords in a local security database in the Cisco router. The NAS authorizes users by comparing their login information with this security database. The network administrator configures user profiles on the local database for each user who may require access.