|  |  | The sensor has the ability to dynamically reconfigure a router's access control lists and shun the source of an attack in real-time. It can instantly stop known bad activities from entering the network. It alerta the user via the director. It utilizes one interface to monitor traffic and another to communicate with the router. It creates an alarm to send back to the director whenever it detects a policy violation through the Cisco router's syslog daemon.