| Network sensors are placed at every protectable entry and exit point of a network, and can be located worldwide in remote sites. Each sensor reports back to a single device, called a director, for centralized administration. All data is encrypted until it reaches the sensor protecting the director. When a known bad activity occurs, the sensors are able to shun those packets from the network. Operators can shun packets on any sensor from the director.