| Cisco's IOS commands are associated with fifteen different levels of privilege. Level one is user mode; users can look at configurations but make no changes. Level two is used with minimal access. Commands such as show, ping, and debug are used for monitoring and testing. Level fifteen is the highest privilege mode; reload, erase NVRAM, erase flash, and shutdown are examples of level fifteen commands. To customize privilege levels, use the privilege level configuration command.