|  |  | Port address translation works very much like NAT, except it assigns a single address to the external interface. PAT can support up to 64,000 hosts with a single IP address. PAT hides internal network information and allows the use of private addresses. PAT works by using the internal host source and destination port number to identify the host connections to and from the external network.