|  |  | Only a finite quantity of IP addresses is in existence and they must be conserved. NAT addresses this need. NAT offers additional network security by hiding information. NAT allows all systems on a LAN to communicate with the Internet through one of a small pool of IP addresses stored on a router. LANs use private IP addresses internally, and the Cisco router administers connections made to the external network.