Handbook of Information Security Management
(Publisher: CRC Press LLC)
Author(s): Hal Tipton and Micki Krause, Consulting Editors
ISBN: 0849399475
Publication Date: 01/01/98

Previous | Table of Contents | Next

Uniqueness of Biometric Organ and Action

Because the purpose of biometric systems is positive identification of personnel, some organizations (e.g., elements of the government) are specifying systems based only on a unique (i.e., no duplicate in the world) physical characteristic. The rationale is that when the base is a unique characteristic, a file match is a positive identification rather than a statement of high probability that this is the right person. Only three physical characteristics or human organs used for biometric identification are unique: the fingerprint, the retina of the eye (i.e., the blood-vessel pattern inside the back of the eyeball), and the iris of the eye (i.e., random pattern of features in the colored portion of the eye surrounding the pupil). These features include freckles, rings, pits, striations, vasculature, coronas, and crypts.

Resistance to Counterfeiting

The ability to detect or reject counterfeit input data is vital to a biometric access control system meeting high security requirements. These include use of rubber, plastic, or even hands or fingers of the deceased in hand or fingerprint systems, and mimicked or recorded input to voice systems. Entertainment media, such as the James Bond or Terminator films, have frequently shown security system failures when the heads or eyes of deceased (i.e., authentic) persons were used to gain access to protected assets or information. Because most of the early biometric identifying verification systems were designed for high security access control applications, failure to detect or reject counterfeit input data was the reason for several system or organization failures. Resistance to counterfeit data remains a criterion of high-quality, high-accuracy systems. However, the proliferation of biometric systems into other non-high-security type applications means that lack of resistance to counterfeiting is not likely to cause the failure of a system in the future.

Reliability

It is vital that biometric identifying verification systems remain in continuous, accurate operation. The system must allow authorized persons access while precluding others, without breakdown or deterioration in performance accuracy or speed. In addition, these performance standards must be sustained without high levels of maintenance or frequent diagnostics and system adjustments.

Data Storage Requirements

Data storage requirements are a far less significant issue today than in the earlier biometric systems when storage media were very expensive. Nevertheless, the size of biometric data files remains a factor of interest. Even with current ultra-high-speed processors, large data files take longer to process than small files, especially in systems that perform full identification, matching the input file against every file in the data base. Biometric file size varies between 9 and 10,000 bytes, with most falling in the 256- to 1,000-byte range.

Enrollment Time

Enrollment time is also a less significant factor today. Early biometric systems sometimes had enrollment procedures requiring many repetitions and several minutes to complete. A system requiring a 5-minute enrollment instead of 2 minutes causes 50 hours of expensive nonproductive time if 1,000 users must be enrolled. Moreover, when line waiting time is considered, the cost increases several times. The accepted standard for enrollment time is 2 minutes per person. Most of the systems in the marketplace today meet this standard.

Intrusiveness of Data Collection

Originally, this factor developed because of user concerns regarding collection of biometric data from inside the body, specifically, the retina inside the eyeball. Early systems illuminated the retina with a red light beam. However, this coincided with increasing public awareness of lasers, sometimes demonstrated as red light beams cutting steel. There has never been an allegation of user injury from retina scanning, but user sensitivity expanded from resistance to red lights intruding inside the body to include any intrusion inside the body. This user sensitivity has now increased to concerns about intrusions into perceived personal space.

Subject and System Contact Requirements

This factor could possibly be considered as a next step or continuation of intrusiveness. Indications are that biometric system users are becoming increasingly sensitive to being required to make firm physical contact with surfaces where up to hundreds of other unknown (to them) persons are required to make contact for biometric data collection. These concerns include voice systems that require holding and speaking into a handset close to the lips.

There seems to be some user feeling that: “if I choose to do something, it is OK, but if an organization, or society, requires me to do the same thing, it is wrong.” Whether or not this makes sense, it is an attitude spreading through society which is having an impact on the use of biometric systems. Systems using video camera data acquisition do not fall into this category.

HISTORICAL BIOMETRIC PROBLEMS

A variety of problems in the field utilization of biometric systems over the past 25 years have been identified. Some have been overcome and are seldom seen today; others still occur. These problems include performance, hardware and software robustness, maintenance requirements, susceptibility to sabotage, perceived health maladies because of usage, private information being made available to management, and skill and cooperation required to use the system.

Performance

Field performance of biometric identifying verification systems is often different than that experienced in manufacturers’ or laboratory tests. There are two ways to avoid being stuck with a system that fails to deliver promised performance. First, limit consideration to technologies and systems that have been tested by an independent, unbiased testing organization. Sandia National Laboratories, located in Albuquerque, New Mexico, has done biometric system testing for the Department of Energy for many years, and some of their reports are available. Second, any system manufacturer or sales representative should be able to provide a list of organizations currently using their system. They should be able to point out those users whose application is similar to that currently contemplated (unless the planned operation is a new and unique application). Detailed discussions, and perhaps a site visit, with current users with similar application requirements should answer most questions and prevent many surprises.

Previous | Table of Contents | Next